From d7cdafe40ae4bc518c303136948020487e060439 Mon Sep 17 00:00:00 2001
From: Philip Lampkin <plampkin@chem.wisc.edu>
Date: Tue, 15 Jun 2021 23:00:04 -0500
Subject: updated fab guide grammar/spelling

---
 fabrication-and-operation-instructions/wpp-fabrication-operation.tex | 5 +++--
 1 file changed, 3 insertions(+), 2 deletions(-)

(limited to 'fabrication-and-operation-instructions/wpp-fabrication-operation.tex')

diff --git a/fabrication-and-operation-instructions/wpp-fabrication-operation.tex b/fabrication-and-operation-instructions/wpp-fabrication-operation.tex
index 4b6761a..86f5f15 100644
--- a/fabrication-and-operation-instructions/wpp-fabrication-operation.tex
+++ b/fabrication-and-operation-instructions/wpp-fabrication-operation.tex
@@ -61,7 +61,7 @@
 \begin{document}
 
 \maketitle
-\textbf{{\centering \Large Wisconsin Photoreactor Platform \\ Fabrication and Operation Guide \\}}
+\textbf{{\centering \huge Wisconsin Photoreactor Platform \\ Fabrication and Operation Guide \\}}
 
 \vspace{10mm} %5mm vertical space
  
@@ -518,6 +518,7 @@ A single 12V 2 A power supply is sufficient to drive 2 WPP devices simultaneousl
 A switch can be installed between the WPP apparatus and power supply to provide power switching.
 A light-blocking shield should be used with WPP devices to limit light exposure.
 
+
 Reaction and photon source cooling is provided by the fan integrated into the base.
 Additional cooling can be achieved through placement of fans above the WPP apparatus or by placing a WPP device on a stir plate within a refrigerator or cold room.
 
@@ -606,7 +607,7 @@ Care must be taken to ensure the light-blocking shield employed adequately block
 
 A 3D printable light-blocking cover module for WPP devices is provided in the 'photoreactor-light-shield' subdirectory of the project repository.
 The WPP light shield prevents direct exposure of users to light emitted by WPP photon sources. 
-We recommend printing the WPP light shield using black filament is recommended to reduce light bounce (Figure 24).
+We recommend printing the WPP light shield using black filament to minimize light bounce (Figure 24).
 
 Use of light-filtering safety glasses alongside a light-blocking shield can provide additional protection from high-intensity light.
 
-- 
cgit v1.2.3

