From f47e1abac351ed10110c9d982aea76ca73dd30a6 Mon Sep 17 00:00:00 2001
From: Blaise Thompson <blaise@untzag.com>
Date: Wed, 31 Jan 2018 18:37:43 -0600
Subject: 2018-01-31 18:37

---
 procedures/chapter.tex | 34 +++++++++++++++++++++++++++++++++-
 1 file changed, 33 insertions(+), 1 deletion(-)

(limited to 'procedures/chapter.tex')

diff --git a/procedures/chapter.tex b/procedures/chapter.tex
index 3cb42bf..4ac67ed 100644
--- a/procedures/chapter.tex
+++ b/procedures/chapter.tex
@@ -1 +1,33 @@
-\chapter{Procedures}
\ No newline at end of file
+\chapter{Procedures}
+
+\section{Aligining TOPAS-C}
+
+\section{Aligning Spitfire PRO}
+
+\section{Air Handling}
+
+\section{Six Month Maintenance}
+
+\section{Tuning MicroHR Monochromator}
+
+Visible Grating.  %
+
+Align the HeNe as perpendicular as possible to the monochromator entrance slit.  %
+
+Move the grating angle until the HeNe falls on the exit slit.  %
+
+Shine a flashlight through the entrance slit and observe the colour on the exit slit: if white,
+then you are at 0-order (0 nm), if red, then you are at 1st order (632.8 nm).  %
+
+Go to 0-order, narrow the slits, and slowly adjust the angle until the HeNe is going through the
+exit slit.  %
+
+Go to Jovin Yvon/utilities and find the motor configuration program.  %
+
+In the Gratings tab, select the 1st grating (1200 line density) and hit Calibrate.  %
+
+In theoretical wavelength, enter 0 nm.  %
+
+In experimental wavelength, enter the wavelength you observe from the control program.  %
+
+Hit set. %
-- 
cgit v1.2.3

