From 7870759e32cc48fc456f07127e841c8a3f3fa236 Mon Sep 17 00:00:00 2001
From: Blaise Thompson <blaise@untzag.com>
Date: Tue, 10 Apr 2018 10:02:48 -0500
Subject: 2018-04-10 10:02

---
 acquisition/chapter.tex | 7 +++++++
 1 file changed, 7 insertions(+)

(limited to 'acquisition/chapter.tex')

diff --git a/acquisition/chapter.tex b/acquisition/chapter.tex
index 5981e22..ab1793d 100644
--- a/acquisition/chapter.tex
+++ b/acquisition/chapter.tex
@@ -474,6 +474,8 @@ They sometimes have an offset, as specified by the autonomic system
 Each hardware can be thought of as a dimension of the MR-CMDS experiment, and scans include a
 specific traversal through this multidimensional space.  %
 
+In this section I briefly discuss PyCMDS' implementation for each type of hardware.  %
+
 \subsection{Hardware inheritance}  % --------------------------------------------------------------
 
 All hardware classes are children of the parent \python{Hardware} class
@@ -492,6 +494,11 @@ methods:
   \item \python{@property units}
 \end{ditemize}
 
+\autoref{aqn:fig:hardware_inheritance} shows the full inheritance tree, including all nine types of
+hardware currently supported by PyCMDS.  %
+In general the nesting is type/model, although there can be additional levels of nesting when
+required, as can be seen in the case of OPA/TOPAS/TOPAS-C and OPA/TOPAS/TOPAS-800.  %
+
 \begin{figure}
 	\includepython{"acquisition/hardware.py"}
   \caption[Parent hardware class.]{
-- 
cgit v1.2.3

