From 9d89c09dfe49aba4c68b6911600715add419babd Mon Sep 17 00:00:00 2001
From: Blaise Thompson <blaise@untzag.com>
Date: Tue, 27 Feb 2018 23:58:32 -0600
Subject: 2018-02-27 23:58

---
 .../delay configuration/delay configuration.tex    | 95 ----------------------
 1 file changed, 95 deletions(-)
 delete mode 100644 instrument/delay configuration/delay configuration.tex

(limited to 'instrument/delay configuration/delay configuration.tex')

diff --git a/instrument/delay configuration/delay configuration.tex b/instrument/delay configuration/delay configuration.tex
deleted file mode 100644
index 08908b8..0000000
--- a/instrument/delay configuration/delay configuration.tex	
+++ /dev/null
@@ -1,95 +0,0 @@
-% document
-\documentclass[11 pt]{report}
-\usepackage[letterpaper, margin=0.75in]{geometry}  % 1 inch margins required
-\usepackage{setspace}
-\usepackage{afterpage}
-\usepackage{color}
-\usepackage{soul}
-\usepackage{array}
-
-% text
-\usepackage[utf8]{inputenc}
-\setlength\parindent{0pt}
-\setlength{\parskip}{1em}
-\usepackage{enumitem}
-\renewcommand{\familydefault}{\sfdefault}
-\newcommand{\RomanNumeral}[1]{\textrm{\uppercase\expandafter{\romannumeral #1\relax}}}
-\usepackage{etoolbox}
-\AtBeginEnvironment{verse}{\singlespacing}
-\AtBeginEnvironment{tabular}{\singlespacing}
-
-% graphics
-\usepackage{graphics}
-\usepackage{graphicx}
-\usepackage{epsfig}
-\usepackage{epstopdf}
-\usepackage{etoc}
-\usepackage{tikz}
-
-% math
-\usepackage{amssymb}
-\usepackage{amsmath}
-\usepackage[cm]{sfmath}
-\DeclareMathOperator{\me}{e}
-
-% hyperref
-\usepackage[colorlinks=true, linkcolor=black, urlcolor=blue, citecolor=black, anchorcolor=black]{hyperref}
-\usepackage[all]{hypcap}  % helps hyperref work properly
-
-% date (http://tex.stackexchange.com/a/237251)
-\def\twodigits#1{\ifnum#1<10 0\fi\the#1}
-\def\mydate{\leavevmode\hbox{\the\year-\twodigits\month-\twodigits\day}}
-
-\begin{document}
-
-{\Huge{new delay configuration}}
-
-last modified \mydate
-
-\dotfill
-
-This is a proposal for a new delay configuration on the fs table.
-
-Priors \& assumptions:
-\begin{itemize}[topsep=-1.5ex, itemsep=0ex, partopsep=0ex, parsep=0ex, label=$\rightarrow$]
-	\item for self-heterodyned experiments, best to keep delay of probe constant (to avoid changes in coupling into the detection optics)
-	\item $z_c$ for fs OPAs is around 25 feet
-\end{itemize}
-
-I propose that the ideal delay configuration would place the long-travel stage on the pump beamline for all experiments. Currently, the long-travel stage is on OPA1. In this configuration we are asked to either change the role of OPAs (pump with OPA1) or scan the probe delay. I'd like to keep the role of the OPAs consistent to make comparison between TREE and self-heterodyned experiments easier.
-
-Since we currently have at-most three beams impingement upon the sample, our three delays \emph{over-constrain} the delay space. Indeed, \texttt{d2} and \texttt{d0} both modify the same logical delay ($\tau_{21}$). \hl{I propose that we switch the locations of the stages.}
-
-\autoref{fig:current} diagrams the current delay configuration.
-
-\begin{figure}[!htb]
-	\centering
-	\includegraphics[width=0.5\linewidth]{IMG_20161221_145528}
-	\caption{current}
-	\label{fig:current}
-\end{figure}
-
-Note that, because \texttt{d0} is now controlling our \textit{pump} line, we want the majority of our dynamic range to be towards \textit{shorter} path lengths. This means that zero delay will place \texttt{d0} in the `far' configuration, somewhat annoyingly. \texttt{d2} will also be `far', but it can be brought a couple inches closer by adjusting the OPA2 beamline one inch inward and OPA1 one inch outward.
-
-\autoref{fig:new} diagrams the proposed delay configuration.
-
-\begin{figure}[!htb]
-	\centering
-	\includegraphics[width=0.5\linewidth]{IMG_20161221_145626}
-	\caption{new}
-	\label{fig:new}
-\end{figure}
-
-This change will add about 10 inches to our path length. This change will be inconsequential for our focusing setup.
-
-This change will make it less convenient to do multi-pass experiments in the long travel stage, but multi-pass is still possible.
-
-In pump-probe geometry, the transmitted split-pump will be blocked (or the beam splitter will be replaced by a mirror).
-
-There should be no need to introduce/remove the OPA2 dogleg in this configuration.
-
-It will remain possible to introduce leakage (800 nm) light into any of the three delay lines.
-
-I think that I can implement this change and re-find zero delay in about one day. We should make this change before carefully re-defining the mask. 
-
-\end{document}
\ No newline at end of file
-- 
cgit v1.2.3

